{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"merged":[[11,2,11,6],[12,2,12,6],[13,1,32,1],[13,2,32,2],[13,3,17,3],[15,5,15,6],[18,3,25,3],[24,5,24,6],[26,3,26,4],[26,5,26,6],[27,3,27,4],[27,5,27,6],[28,3,28,4],[29,3,30,3],[30,5,30,6],[31,3,32,3],[33,1,48,1],[33,2,43,2],[33,3,33,4],[34,3,34,4],[35,3,35,4],[36,3,36,4],[36,5,36,6],[37,3,39,3],[40,3,41,3],[41,5,41,6],[42,3,43,3],[42,5,42,6],[43,5,43,6],[44,2,47,2],[45,3,45,4],[46,3,46,4],[47,3,47,4],[47,5,47,6],[48,2,48,4],[50,1,52,1],[50,2,52,6],[53,1,53,3],[54,1,54,3]],"flags":["formulas_cached_only"]}
[]
[]
[null,"Wavelength Convertor　Questionarrire"]
[]
[null,"Customer code"]
[null,"Customer name"]
[null,"Corresponding person"]
[null,"Date"]
[]
[]
[]
[null,"Application"]
[null,"Conversion Type"]
[null,"Laser","FH","CW","Center Wavelength",null,"nm"]
[{"$nulls":4},"Bandwidth",null,"nm"]
[{"$nulls":4},"M2"]
[{"$nulls":4},"Extinction Ratio",null,"dB"]
[{"$nulls":4},"Power",null,"W"]
[{"$nulls":3},"Pulsed","Center Wavelength",null,"nm"]
[{"$nulls":4},"Peak Power",null,"kW"]
[{"$nulls":4},"Average Power",null,"W"]
[{"$nulls":4},"Pulse Energy",null,"mJ"]
[{"$nulls":4},"Pulse rep. rate",null,"kHz"]
[{"$nulls":4},"Pulse width",null,"ns"]
[{"$nulls":4},"Pulse Shape"]
[{"$nulls":4},"Bandwidth (FWHM)",null,"nm"]
[{"$nulls":3},"Isolator mounted?"]
[{"$nulls":3},"Polarization (randam or linear)"]
[{"$nulls":3},"Extenction ratio",null,null,"dB"]
[{"$nulls":3},"Output Fiber","MFD",null,"um"]
[{"$nulls":4},"NA"]
[{"$nulls":3},"Collimator","Beam diameter",null,"mm"]
[{"$nulls":4},"Beam divergence（at beam waist）",null,"mrad"]
[null,"Wavelength Convertor","Converted Output","Wavelength",null,null,"nm"]
[{"$nulls":3},"Expected Output or Conversion efficiency",null,null,"W"]
[{"$nulls":3},"Power stability",null,null,"%"]
[{"$nulls":3},"Mode shape or M2"]
[{"$nulls":3},"Collimated ","Bema waist size",null,"um"]
[{"$nulls":4},"Beam divergence（at beam waist）",null,"mrad"]
[{"$nulls":4},"Pointing Stability",null,"mrad"]
[{"$nulls":3},"Fiber","MFD",null,"um"]
[{"$nulls":4},"NA"]
[{"$nulls":3},"Connector","Type"]
[{"$nulls":4},"AR coating?"]
[null,null,"Package","Max. Size","(L) x (W) x (T)",null,"mm"]
[{"$nulls":3},"Weight",null,null,"g"]
[{"$nulls":3},"Consumption power",null,null,"W"]
[{"$nulls":3},"Mounting base"]
[null,null,"Quantity",{"$nulls":3},"pc"]
[]
[null,"Other Requests"]
[]
[]
[null,"Your budget for this request",null,null,"(Ex. Approximately 1M JPY)"]
[null,"Quantities of future demand",null,null,"(Ex. 10 pieces/year, 50 pieces/year)"]